#Chat script for China Mobile, used SIMCOM sim4100 TD module.
TIMEOUT 15
ABORT "DELAYED"
ABORT "BUSY"
ABORT "ERROR"
ABORT "NO DIALTONE"
ABORT "NO CARRIER"
TIMEOUT 40
'' \rAT
OK ATS0=0
OK ATE0V1
#OK AT+CGDCONT=1,"IP","CMNET"
OK    AT+CGDCONT=1,"IP","3GNET"
#OK AT+CGEQREQ=1,2,128,384,,,0,,,,,,
#OK    ATDT*99*1#
OK    ATDT*99#
CONNECT
