#! /bin/sh

/bin/mount -a

echo "
            _ _ _ _ _ _ _ _ _ _ _ _
            \  _  _   _  _ _ ___
            / /__/ \ |_/
           / __   /  -  _ ___
          / /  / /  / /
  _ _ _ _/ /  /  \_/  \_ ______
___________\___\__________________
"
for initscript in /etc/init.d/S[0-9][0-9]*
do
	if [ -x $initscript ] ;
	then
		echo "[RCS]: $initscript"
		$initscript
	fi
done

/sbin/sysctl -p /etc/sysctl.conf

cd /ko
./load3521d -i

telnetd

chown root:root /var/empty
/usr/local/sbin/sshd

#UART3
#himm 0x120F0100 1
#himm 0x120F0100 1

#UART1
himm 0x120F00F8 1
himm 0x120F00FC 1

#I2S
himm 0x120F00A0 1
himm 0x120F00A4 1
himm 0x120F00A8 1
himm 0x120F00AC 1
himm 0x120F00B0 1
himm 0x120F00B4 1
himm 0x120F00B8 1
himm 0x120F00BC 1

#QOS
himm 0x12120084 0x66663666

#i2c
himm 0x120F00E0 1
himm 0x120F00E4 1

/link/shell/init.sh


